
Sysbench 0.9.1d result file created Mon Jul 21 21:36:20 1997
Machine name    - CCK Technologies Pentium 133
Manufacturer    - CCK Technologies
Motherboard     - ABit SM5
Chipset         - Intel 430VX
Processor       - Intel Pentium-S 133
External cache  - 512K
Graphics card   - Asus V775V2C
Disk Controller - On-board EIDE
Machine data
Coprocessor     = Yes
RAM             = 32.00 MB
Priority        = Dynamic
Maxwait         = 2
Timeslice       = (32,32)
Swap file size  = 20.00MB
  ...initially  = 20.00MB
Video data
Resolution      = 1024x768x16 bits/pixel
Number planes   = 0
Screen Access   = Direct
Bank Switched   = No
Bytes/scanline  = 2048
Aperture size   = 2097152
Manufact. code  = 8
Chipset code    = 16
 Graphics
   BitBlt S->S cpy       :       51.577    Mpixels/s
   BitBlt M->S cpy       :        6.477    Mpixels/s
   Filled Rectangle      :      159.756    Mpixels/s
   Pattern Fill          :      161.309    Mpixels/s
   Vertical Lines        :        9.828    Mpixels/s
   Horizontal Lines      :       14.781    Mpixels/s
   Diagonal Lines        :       11.496    Mpixels/s
   Text Render           :       11.309    Mpixels/s
   ------------------------------------------------------------
   Total                 :       50.796    PM-marks
 CPU integer
   Dhrystone             :      105.738    VAX 11/780 MIPS
   Hanoi                 :       84.519    moves/25 usec
   Heapsort              :       61.242    MIPS
   Sieve                 :      119.253    MIPS
   ------------------------------------------------------------
   Total                 :       95.670    CPUint-marks
 CPU float
   Linpack               :        9.271    MFLOPS
   Flops                 :       20.859    MFLOPS
   Fast Fourier Tr.      :       15.494    VAX FFT's
   ------------------------------------------------------------
   Total                 :       16.650    CPUfloat-marks
 Direct Interface to video extensions - DIVE
   Video bus bandw.      :       53.864    MB/s
   DIVE fun              :      188.678    fps at 640x480x256
   M->S, DD,   1.00:1    :      184.069    fps at 640x480x256
   ------------------------------------------------------------
   Total                 :       69.105    DIVE-marks
 File I/O - cache read - Drive D:
   4Kb seq.   N     N    :     3355.853    KB/sec
   4Kb seq.   N     Y    :     3797.600    KB/sec
   4Kb random N     N    :      391.791    KB/sec
   4Kb random N     Y    :      388.326    KB/sec
   4Kb seq.   Y     N    :     1055.655    KB/sec
   4Kb seq.   Y     Y    :     3436.034    KB/sec
   4Kb random Y     N    :      112.620    KB/sec
   4Kb random Y     Y    :      121.615    KB/sec
   8Kb seq.   N     N    :     3724.955    KB/sec
   8Kb seq.   N     Y    :     4036.228    KB/sec
   8Kb random N     N    :      720.000    KB/sec
   8Kb random N     Y    :      704.158    KB/sec
   8Kb seq.   Y     N    :     1100.605    KB/sec
   8Kb seq.   Y     Y    :     4014.917    KB/sec
   8Kb random Y     N    :      205.642    KB/sec
   8Kb random Y     Y    :      697.067    KB/sec
   16K seq.   N     N    :     1912.673    KB/sec
   16K seq.   N     Y    :     4088.617    KB/sec
   16K random N     N    :     1305.970    KB/sec
   16K random N     Y    :     1256.533    KB/sec
   16K seq.   Y     N    :     1192.632    KB/sec
   16K seq.   Y     Y    :     4007.459    KB/sec
   16K random Y     N    :      373.524    KB/sec
   16K random Y     Y    :     1275.733    KB/sec
   32K seq.   N     N    :     3497.570    KB/sec
   32K seq.   N     Y    :     5066.098    KB/sec
   32K random N     N    :     2118.400    KB/sec
   32K random N     Y    :     2044.776    KB/sec
   32K seq.   Y     N    :     3398.721    KB/sec
   32K seq.   Y     Y    :     5040.512    KB/sec
   32K random Y     N    :     2048.000    KB/sec
   32K random Y     Y    :     2033.031    KB/sec
   64K seq.   N     N    :     6079.212    KB/sec
   64K seq.   N     Y    :     2587.107    KB/sec
   64K random N     N    :     3323.733    KB/sec
   64K random N     Y    :     2938.166    KB/sec
   64K seq.   Y     N    :     1406.360    KB/sec
   64K seq.   Y     Y    :     1615.344    KB/sec
   64K random Y     N    :     1280.000    KB/sec
   64K random Y     Y    :     1655.467    KB/sec
   ------------------------------------------------------------
   Total                 :     2235.218    File I/O-marks
 Memory
   5    kB copy          :      397.651    MB/s
   10   kB copy          :      130.035    MB/s
   20   kB copy          :       67.253    MB/s
   40   kB copy          :       63.095    MB/s
   80   kB copy          :       63.036    MB/s
   160  kB copy          :       58.802    MB/s
   320  kB copy          :       57.749    MB/s
   640  kB copy          :       49.350    MB/s
   1280 kB copy          :       44.543    MB/s
   5    kB read          :      159.085    MB/s
   10   kB read          :      121.080    MB/s
   20   kB read          :      106.129    MB/s
   40   kB read          :      106.235    MB/s
   80   kB read          :      106.263    MB/s
   160  kB read          :      103.418    MB/s
   320  kB read          :       82.775    MB/s
   640  kB read          :       76.855    MB/s
   1280 kB read          :       70.776    MB/s
   5    kB write         :       84.310    MB/s
   10   kB write         :       84.272    MB/s
   20   kB write         :       84.313    MB/s
   40   kB write         :       84.313    MB/s
   80   kB write         :       84.260    MB/s
   160  kB write         :       84.250    MB/s
   320  kB write         :       83.872    MB/s
   640  kB write         :       83.935    MB/s
   1280 kB write         :       83.894    MB/s
   ------------------------------------------------------------
   Total                 :       74.884    Mem-marks
 Disk I/O disk 1:  1547 MB - Seagate ST31621A
   Avg. data access time :       17.300    ms
   Cache/Bus xfer rate   :        6.106    MB/s
   Average Transfer rate :        4.775    MB/s
   Disk use CPU load     :       75.000    percent
   ------------------------------------------------------------
   Total                 :       34.422    Disk I/O-marks
 CD-ROM I/O disk 1:   515 MB - Panasonic 8x CD Rom
   Avg. data access time :      116.300    ms
   Average Transfer rate :     1197.000    KB/s
   CD-ROM use CPU load   :       70.000    percent
   ------------------------------------------------------------
   Total                 :       61.505    CD I/O-marks
