
Sysbench 0.9.1d result file created Tue Jul 22 00:38:39 1997
Machine name    - CCK Technologies Pentium 133
Manufacturer    - CCK Technologies
Motherboard     - ABit SM5
Chipset         - Intel 430VX
Processor       - Intel Pentium-S 133
External cache  - 512K
Graphics card   - Asus V775V2C
Disk Controller - On-board EIDE
Machine data
Coprocessor     = Yes
RAM             = 32.00 MB
Priority        = Dynamic
Maxwait         = 1
Timeslice       = (32,32)
Swap file size  = 20.00MB
  ...initially  = 20.00MB
Video data
Resolution      = 1024x768x16 bits/pixel
Number planes   = 0
Screen Access   = Direct
Bank Switched   = No
Bytes/scanline  = 2048
Aperture size   = 2097152
Manufact. code  = 8
Chipset code    = 16
 Graphics
   BitBlt S->S cpy       :       51.577    Mpixels/s
   BitBlt M->S cpy       :        6.582    Mpixels/s
   Filled Rectangle      :      159.809    Mpixels/s
   Pattern Fill          :      161.309    Mpixels/s
   Vertical Lines        :        9.700    Mpixels/s
   Horizontal Lines      :       14.781    Mpixels/s
   Diagonal Lines        :       11.562    Mpixels/s
   Text Render           :       11.315    Mpixels/s
   ------------------------------------------------------------
   Total                 :       50.814    PM-marks
 CPU integer
   Dhrystone             :      105.748    VAX 11/780 MIPS
   Hanoi                 :       84.814    moves/25 usec
   Heapsort              :       62.399    MIPS
   Sieve                 :      119.508    MIPS
   ------------------------------------------------------------
   Total                 :       96.017    CPUint-marks
 CPU float
   Linpack               :        9.347    MFLOPS
   Flops                 :       20.858    MFLOPS
   Fast Fourier Tr.      :       16.031    VAX FFT's
   ------------------------------------------------------------
   Total                 :       16.793    CPUfloat-marks
 Direct Interface to video extensions - DIVE
   Video bus bandw.      :       53.840    MB/s
   DIVE fun              :      188.541    fps at 640x480x256
   M->S, DD,   1.00:1    :      184.122    fps at 640x480x256
   ------------------------------------------------------------
   Total                 :       69.102    DIVE-marks
 File I/O - cache read - Drive D:
   4Kb seq.   N     N    :     2354.108    KB/sec
   4Kb seq.   N     Y    :     6000.267    KB/sec
   4Kb random N     N    :      384.800    KB/sec
   4Kb random N     Y    :      413.067    KB/sec
   4Kb seq.   Y     N    :      890.517    KB/sec
   4Kb seq.   Y     Y    :     5149.333    KB/sec
   4Kb random Y     N    :      109.457    KB/sec
   4Kb random Y     Y    :      124.000    KB/sec
   8Kb seq.   N     N    :     3980.020    KB/sec
   8Kb seq.   N     Y    :     6018.657    KB/sec
   8Kb random N     N    :      707.200    KB/sec
   8Kb random N     Y    :      777.067    KB/sec
   8Kb seq.   Y     N    :      712.281    KB/sec
   8Kb seq.   Y     Y    :     6019.733    KB/sec
   8Kb random Y     N    :      211.858    KB/sec
   8Kb random Y     Y    :      774.400    KB/sec
   16K seq.   N     N    :     1922.216    KB/sec
   16K seq.   N     Y    :     5937.067    KB/sec
   16K random N     N    :     1305.600    KB/sec
   16K random N     Y    :     1395.615    KB/sec
   16K seq.   Y     N    :     1266.525    KB/sec
   16K seq.   Y     Y    :     5915.733    KB/sec
   16K random Y     N    :      385.197    KB/sec
   16K random Y     Y    :     1394.456    KB/sec
   32K seq.   N     N    :     3508.221    KB/sec
   32K seq.   N     Y    :     5768.533    KB/sec
   32K random N     N    :     2164.179    KB/sec
   32K random N     Y    :     2250.667    KB/sec
   32K seq.   Y     N    :     3255.467    KB/sec
   32K seq.   Y     Y    :     5755.733    KB/sec
   32K random Y     N    :     2013.867    KB/sec
   32K random Y     Y    :     2253.731    KB/sec
   64K seq.   N     N    :     6287.540    KB/sec
   64K seq.   N     Y    :     2767.591    KB/sec
   64K random N     N    :     3060.406    KB/sec
   64K random N     Y    :     3204.267    KB/sec
   64K seq.   Y     N    :     1363.148    KB/sec
   64K seq.   Y     Y    :     1656.310    KB/sec
   64K random Y     N    :     1286.136    KB/sec
   64K random Y     Y    :     1664.000    KB/sec
   ------------------------------------------------------------
   Total                 :     2560.224    File I/O-marks
 Memory
   5    kB copy          :      455.780    MB/s
   10   kB copy          :      128.759    MB/s
   20   kB copy          :       67.260    MB/s
   40   kB copy          :       58.929    MB/s
   80   kB copy          :       58.889    MB/s
   160  kB copy          :       55.669    MB/s
   320  kB copy          :       55.676    MB/s
   640  kB copy          :       47.216    MB/s
   1280 kB copy          :       44.792    MB/s
   5    kB read          :      161.573    MB/s
   10   kB read          :      120.266    MB/s
   20   kB read          :      106.191    MB/s
   40   kB read          :       96.230    MB/s
   80   kB read          :       91.823    MB/s
   160  kB read          :       98.306    MB/s
   320  kB read          :       82.686    MB/s
   640  kB read          :       75.606    MB/s
   1280 kB read          :       70.776    MB/s
   5    kB write         :       84.260    MB/s
   10   kB write         :       84.260    MB/s
   20   kB write         :       84.317    MB/s
   40   kB write         :       84.295    MB/s
   80   kB write         :       84.294    MB/s
   160  kB write         :       84.250    MB/s
   320  kB write         :       83.935    MB/s
   640  kB write         :       83.935    MB/s
   1280 kB write         :       83.926    MB/s
   ------------------------------------------------------------
   Total                 :       75.521    Mem-marks
 Disk I/O disk 1:  1547 MB - Seagate ST31621A
   Avg. data access time :       17.200    ms
   Cache/Bus xfer rate   :       12.378    MB/s
   Average Transfer rate :        5.626    MB/s
   Disk use CPU load     :       11.000    percent
   ------------------------------------------------------------
   Total                 :       46.208    Disk I/O-marks
 CD-ROM I/O disk 1:   515 MB - Panasonic 8x CD Rom
   Avg. data access time :      119.200    ms
   Average Transfer rate :     1205.000    KB/s
   CD-ROM use CPU load   :       25.000    percent
   ------------------------------------------------------------
   Total                 :       62.232    CD I/O-marks
