### Sysbench 0.9.1d results

#### CPU Integer tests

CPU | Brand/Board | Chip set | Bios | Cache | Cache Type | Dhrystone | Hanoi | Heapsort | Sieve | CpuI-marks
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Intel Pentium-S 133 | CCK Technologies/ABit SM5 | Intel 430VX | Award | 512K |  | 105.748 | 84.814 | 62.399 | 119.508 | 96.017

#### CPU Floating Point tests

CPU | Brand/Board | Chip set | Bios | Cache | Cache Type | LinPack | Flops | FFT | CpuF-marks
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Intel Pentium-S 133 | CCK Technologies/ABit SM5 | Intel 430VX | Award | 512K |  | 9.347 | 20.858 | 16.031 | 16.793

#### DIVE tests

CPU | Vid Bus | Vid Card | Chip Set | Vid Mem | Video Bus Bandwidth | DIVE fun | M->S DD 1.00:1 | Dive-marks
--- | --- | --- | --- | --- | --- | --- | --- | ---
Intel Pentium-S 133 | ISA/PCI | Asus V775V2 | S3 Unknown | 2 MB | 53.840 | 188.541 | 184.122 | 69.102

#### Video tests

#### 1024x768x65536

CPU | Vid Bus | Vid Card | Chip Set | Vid Mem | BitBlt S->S Copy | BitBlt M->S Copy | Filled Rect. | Pattern Fill | Vert. Lines | Horiz. Lines | Diag. Lines | Text Render | PM-marks
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Intel Pentium-S 133 | ISA/PCI | Asus V775V2 | S3 Unknown | 2 MB | 51.577 | 6.582 | 159.809 | 161.309 | 9.700 | 14.781 | 11.562 | 11.315 | 50.814

#### Disk tests

CPU | Brand/Board | Bus | Controller | Drive | Avg. Data Access time | Cache/Bus xfer | Avg. Transfer | Disk use CPU load | DiskIO-marks
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Intel Pentium-S 133 | CCK Technologies/ABit SM5 | ISA/PCI | On-board EIDE | Seagate ST31621A | 17.200 | 12.378 | 5.626 | 11.000 | 46.208

#### CD-ROM tests

CPU | Brand/Board | Bus | Controller | Drive | Avg. Data Access time | Avg. Transfer | CD use CPU load | CD I/O-marks
--- | --- | --- | --- | --- | --- | --- | --- | ---
Intel Pentium-S 133 | CCK Technologies/ABit SM5 | ISA/PCI | On-board EIDE | Panasonic 8x CD Rom | 119.200 | 1205.000 | 25.000 | 62.232

For those who prefer complete details, please click here.